****

**Grave Marker Checklist**

|  |  |
| --- | --- |
| Upright: Grave marker is of unpolished natural stone, measuring no larger than 2 ft in height with combined width and height totaling no more than 4 ft.Foundations: If the grave marker has a concrete foundation, the foundation must be flush with the ground and not extend beyond the grave maker more than four inches on any side. The existing grade shall be maintained. | **Unpolished Natural Stone? Y/N**      **Height:**      **Combined Width and Height:**      **Description of Foundation:**      **Other Description:**       |
| Ground Level:Ground level markers shall be flush with the ground and no larger than six (6) by ten (10) inches. | **Describe Ground Level Marker:** |
| The stone shall be of neutral coloring of gray, beige or sand and of earth and brown tones. | **Color:**       |
| Proposed engraving to be done directly on the stone; free of metal, photos, ornamentation, or modern trimmings. | **Description of engraving and any other proposed stone enhancements:**      |
| How will marker be transported and installed?  |       |

Completed applications can be brought to the Mosier City Hall at 208 Washington St. in Mosier, mailed to PO Box 456 Mosier, OR 97040, or emailed to mosiercityhall@cityofmosier.com.